## Carlton County and Fond du Lac Reservation Aggregate Resource Evaluation - Aggregate Potential - Sand and Gravel Potential - carlsgp

This page last updated: 2009
Metadata created using Minnesota Geographic Metadata Guidelines

### Metadata Summary

Originator | Minnesota Department of Natural Resources, Division of Lands and Minerals, Mineral Potential Evaluation Section
Abstract | This dataset consists of information about the geology, geological characteristics, and sand and gravel potential of 256 map units. Five fields relate to the surficial geology of the map unit, including a unique map unit id, sediment, landform, surficial geology description, and dominant lithology. Five fields relate to sand and gravel characteristics, including probability, quality, texture, overburden thickness, deposit size, and sand and gravel thickness. These characteristics were used to calculate the aggregate potential of the map unit for sand and gravel.
Browse Graphic | none available
Time Period of Content Date | 2009
Currentness Reference | Data were gathered in the spring and fall of 2008 and the spring of 2009. Data were compiled and interpreted in the winter of 2008 through the spring of 2009.
Access Constraints | Acknowledgement of the Minnesota Department of Natural Resources is appreciated for products derived from these data.
Use Constraints | Acknowledgement of the MN DNR is appreciated in products derived from these data.
Distributor Organization | Minnesota Department of Natural Resources, Division of Lands and Minerals
Ordering Instructions | The Aggregate Resource Mapping Program's spatial datasets for Carlton County and the Fond du Lac Reservation are included in the file carlton_aggregate_data.zip, accessible from the MN DNR Aggregate Mapping web page: http://www.dnr.state.mn.us/lands_minerals/aggregate_maps/completed/index.html The spatial datasets are also available as shapefiles and a file geodatabase stored at drive:\data\resource on the associated CD (where 'drive' is the CD reader or writer drive on the PC). The spatial datasets include: sand and gravel potential, crushed stone potential, field observations, mining pits, depleted mining lands, Minnesota Geological Survey (MGS) County Well Index (CWI) data points, sieve analysis table of selected field observations, MGS CWI stratigraphy table, and Mn/DOT ASIS pit quality table. Selected aggregate resource datasets from this project can also be viewed in the Aggregate Resource Mapping Program's Aggregate Mapper at: http://www.dnr.state.mn.us/lands_minerals/aggregate_maps/online_maps/index.html Aggregate Mapper allows users the ability to work with the aggregate resource data without having to download additional software. The site can display spatial and tabular aggregate resource data such as sand and gravel potential, crushed stone potential, field observations, mining pits, and depleted mining lands. This information can be overlaid on a variety of base map information from Web Mapping Services (WMS) sources like; 1:24,000-scale DRGs (digital topographic maps), 1991 black-and-white air photos, and 2008 Farm Service Agency color air photos.
Online Linkage | Click here to download data. (See Ordering Instructions above for details.) By clicking here, you agree to the notice in "Distribution Liability" in Section 6 of this metadata.

### Full Metadata

## Carlton County and Fond du Lac Reservation Aggregate Resource Evaluation - Aggregate Potential - Sand and Gravel Potential - carlsgp

Go to Section:
1. Identification Information
2. Data Quality Information
3. Spatial Data Organization Information
4. Spatial Reference Information
5. Entity and Attribute Information
6. Distribution Information
7. Metadata Reference Information

Section 1 | Identification Information |  | Top of page
Originator | Minnesota Department of Natural Resources, Division of Lands and Minerals, Mineral Potential Evaluation Section
Title | Carlton County and Fond du Lac Reservation Aggregate Resource Evaluation - Aggregate Potential - Sand and Gravel Potential - carlsgp
Abstract | This dataset consists of information about the geology, geological characteristics, and sand and gravel potential of 256 map units. Five fields relate to the surficial geology of the map unit, including a unique map unit id, sediment, landform, surficial geology description, and dominant lithology. Five fields relate to sand and gravel characteristics, including probability, quality, texture, overburden thickness, deposit size, and sand and gravel thickness. These characteristics were used to calculate the aggregate potential of the map unit for sand and gravel.
Purpose | To summarize the geological characteristics, surficial geology, and aggregate potential (sand, gravel) of the different units. To help categorize the geological characteristics and incorporate them into a model to help determine the aggregate potential of the deposit.
Time Period of Content Date | 2009
Currentness Reference | Data were gathered in the spring and fall of 2008 and the spring of 2009. Data were compiled and interpreted in the winter of 2008 through the spring of 2009.
Progress | Complete
Maintenance and Update Frequency | None planned
Spatial Extent of Data | Carlton County, Minnesota including the Fond du Lac Reservation
Bounding Coordinates | -93.06 -92.29 46.88 46.42
Place Keywords | Carlton County, Minnesota, Fond du Lac Reservation
Theme Keywords | aggregate potential, sand and gravel, surficial geology, geological characteristics, probability, quality
Theme Keyword Thesaurus |
Access Constraints | Acknowledgement of the Minnesota Department of Natural Resources is appreciated for products derived from these data.
Use Constraints | Acknowledgement of the MN DNR is appreciated in products derived from these data.
Contact Person Information | Aggregate Resource Mapping Program, Industrial Minerals Geologist or GIS Specialist Minnesota Department of Natural Resources, Division of Lands and Minerals 500 Lafayette Road St. Paul, MN 55155-4045 Phone: 651-259-5959 FAX: 651-296-5939 E-mail: aggregatemap@state.mn.us
Browse Graphic | none available
Browse Graphic File Description |
Associated Data Sets | The Aggregate Resource Mapping Program's spatial datasets for Carlton County and the Fond du Lac Reservation are included in the file carlton_aggregate_data.zip, accessible from the MN DNR Aggregate Mapping web page: http://www.dnr.state.mn.us/lands_minerals/aggregate_maps/completed/index.html The spatial datasets are also available as shapefiles and a file geodatabase stored at drive:\data\resource on the associated CD (where 'drive' is the CD reader or writer drive on the PC). The spatial datasets include: sand and gravel potential, crushed stone potential, field observations, mining pits, depleted mining lands, Minnesota Geological Survey (MGS) County Well Index (CWI) data points, sieve analysis table of selected field observations, MGS CWI stratigraphy table, and Mn/DOT ASIS pit quality table. Selected aggregate resource datasets from this project can also be viewed in the Aggregate Resource Mapping Program's Aggregate Mapper at: http://www.dnr.state.mn.us/lands_minerals/aggregate_maps/online_maps/index.html Aggregate Mapper allows users the ability to work with the aggregate resource data without having to download additional software. The site can display spatial and tabular aggregate resource data such as sand and gravel potential, crushed stone potential, field observations, mining pits, and depleted mining lands. This information can be overlaid on a variety of base map information from Web Mapping Services (WMS) sources like; 1:24,000-scale DRGs (digital topographic maps), 1991 black-and-white air photos, and 2008 Farm Service Agency color air photos.
Section 2 | Data Quality Information | Top of full metadata | Top of page
Attribute Accuracy |
Logical Consistency | Overshoots and undershoots were fixed using topology in ArcGIS 9.3, thus the lines have been checked and completed.
Completeness | The sand and gravel potential map units were delineated by the interpretation of aerial photographs at a 1:40000 scale. These interpretations were plotted on 1:24000 USGS topographic maps. These delineations and unit descriptions were field checked and revised. The final coverage was digitized onscreen using ArcGIS 9.3 with USGS DOQs (at a scale of 1:12000) and USGS DRGs (at a scale of 1:24000) as the spatially registered backdrops. This was a reconnaissance-scale survey and was mapped at 1:50000.
Horizontal Positional Accuracy | 1:50000
Vertical Positional Accuracy | Not applicable.
Lineage | Color, color-infrared (CIR), and black-and-white aerial photographs were used to delineate geological landforms and aggregate resources. Sources include; Stereoscopic pairs of color infrared aerial photographs (NAPP, 9in x 9in at 1:40000 scale, April 1991 and April 1992); On-screen landform analysis was used with FSA (Farm Services Administration) Color Aerial Photography collected from the following years, with their associated pixel resolution in parenthesis; 2003-04 (1 meter), 2005 (10 meter), 2006 (10 meter), 2008 (1 meter); and FSA CIR (Color Infrared) Imagery collected in 2008 (1 meter). Aerial photographic interpretation was completed with a glacial mapping technique known as the landsystems approach. This technique relies on the principle that depositional glacial landforms are composed of a predictable range of sediments, some consisting of sorted sand and gravel and others consisting of silts, clays, or unsorted materials. In addition to the landsystems approach, several other general characteristics helped determine the nature of the material, such as tonal contrasts, texture, context, shape, size, trend, association, and patterns. These characteristics can help determine the properties of the surface material (e.g., certain vegetation grows on well drained soils such as sand and gravel, which on an aerial photograph has a distinctive texture, tone, pattern, etc.). The landform recognition approach (part of the landsystems approach) was also used when interpreting the topography within Carlton County and the Fond du Lac Reservation. Glacial landforms have distinct and unique shapes and patterns that can be observed in their topographic expression. Topographic maps (USGS 1:24000), digital elevation models, and shaded relief maps were all used to help delineate these sand and gravel bearing features. The topographic expression of a feature can also be observed by looking at the distribution of lakes and wetlands. For example, a string of lakes and/or wetlands may be the signature of a glacial outwash channel or collapsed channel, which may host sand or gravel deposits. Several aggregate bearing features were located using this technique (outwash channels, collapsed channels, glaciofluvial fans, eskers, and terraces).
Source Scale Denominator | 50000
Section 3 | Spatial Data Organization Information | Top of full metadata | Top of page
Native Data Set Environment | ArcGIS 9.3 from ESRI
Geographic Reference for Tabular Data |
Spatial Object Type | Vector
Vendor Specific Object Types | Polygon
Tiling Scheme | Carlton County and Fond du Lac Reservation
Section 4 | Spatial Reference Information | Top of full metadata | Top of page
Horizontal Coordinate Scheme | UTM
Ellipsoid | GRS80
Horizontal Datum | NAD83
Horizontal Units | Meters
Distance Resolution |
Altitude Datum | Not applicable
Depth Datum | Not applicable
UTM Zone Number | 15E
Section 5 | Entity and Attribute Information | Top of full metadata | Top of page
Entity and Attribute Overview | The polygons were delineated to represent geological features, geological characteristics, and aggregate potential for sand and gravel.
Entity and Attribute Detailed Citation | carlsgp_att.htm Attribute values can be found in the following table: carlsgp_att.htm. If this table hotlink cannot be found by your browser, you can find this file stored in the same location (i.e., drive:\docs) as this metadata record.
Section 6 | Distribution Information | Top of full metadata | Top of page
Publisher | Minnesota Department of Natural Resources, Division of Lands and Minerals, Mineral Potential Evaluation Section
Publication Date | 2009
Contact Person Information | Aggregate Resource Mapping Program Industrial Minerals Geologist or GIS Specialist Minnesota Department of Natural Resources, Division of Lands and Minerals 500 Lafayette Road St. Paul, MN 55155-4045 Phone: 651-259-5959 FAX: 651-296-5939 E-mail: aggregatemap@state.mn.us
Distributor's Data Set Identifier | Carlton County and Fond du Lac Reservation Aggregate Resource Evaluation
Distribution Liability | The Minnesota Department of Natural Resources makes no representation or warranties, express or implied, with respect to the reuse of data provided herewith, regardless of its format or the means of its transmission. There is no guarantee or representation to the user as to the accuracy, currency, suitability, or reliability of this data for any purpose. The user accepts the data 'as is', and assumes all risks associated with its use. By accepting this data, the user agrees not to transmit this data or provide access to it or any part of it to another party unless the user shall include with the data a copy of this disclaimer. The Minnesota Department of Natural Resources assumes no responsibility for actual or consequential damage incurred as a result of any user's reliance on this data.
Transfer Format Name |
Transfer Format Version Number |
Transfer Size | mb for data, mb for associated maps
Ordering Instructions | The Aggregate Resource Mapping Program's spatial datasets for Carlton County and the Fond du Lac Reservation are included in the file carlton_aggregate_data.zip, accessible from the MN DNR Aggregate Mapping web page: http://www.dnr.state.mn.us/lands_minerals/aggregate_maps/completed/index.html The spatial datasets are also available as shapefiles and a file geodatabase stored at drive:\data\resource on the associated CD (where 'drive' is the CD reader or writer drive on the PC). The spatial datasets include: sand and gravel potential, crushed stone potential, field observations, mining pits, depleted mining lands, Minnesota Geological Survey (MGS) County Well Index (CWI) data points, sieve analysis table of selected field observations, MGS CWI stratigraphy table, and Mn/DOT ASIS pit quality table. Selected aggregate resource datasets from this project can also be viewed in the Aggregate Resource Mapping Program's Aggregate Mapper at: http://www.dnr.state.mn.us/lands_minerals/aggregate_maps/online_maps/index.html Aggregate Mapper allows users the ability to work with the aggregate resource data without having to download additional software. The site can display spatial and tabular aggregate resource data such as sand and gravel potential, crushed stone potential, field observations, mining pits, and depleted mining lands. This information can be overlaid on a variety of base map information from Web Mapping Services (WMS) sources like; 1:24,000-scale DRGs (digital topographic maps), 1991 black-and-white air photos, and 2008 Farm Service Agency color air photos.
Online Linkage | Click here to download data. (See Ordering Instructions above for details.) By clicking here, you agree to the notice in "Distribution Liability" above.
Section 7 | Metadata Reference Information | Top of full metadata | Top of page
Metadata Date | 2009
Contact Person Information | Aggregate Resource Mapping Program, Industrial Minerals Geologist or GIS Specialist Minnesota Department of Natural Resources, Division of Lands and Minerals 500 Lafayette Road St. Paul, MN 55155-4045 Phone: 651-259-5959 FAX: 651-296-5939 E-mail: aggregatemap@state.mn.us
Metadata Standard Name | Minnesota Geographic Metadata Guidelines
Metadata Standard Version | 1.2
Metadata Standard Online Linkage | http://www.lmic.state.mn.us/gc/stds/metadata.htm

This page last updated: 2009